**COBRA-TF Residual Formulation Solid Liquid Coupling**

**C. Dances1, M. Avramova1 and V. Mousseau2**

1: Department of Mechanical and Nuclear Engineering, The Pennsylvania State University, 137 Reber BuildingUniversity Park, PA 16802, USA

2:Computer Science Research Institute, Sandia National Labs, 1450 Innovation Parkway, Albuquerque, NM 87123, USA

[cad39@psu.edu](mailto:cad39@psu.edu), [mna109@psu.edu](mailto:mna109@psu.edu), [vamouss@sandia.gov](mailto:vamouss@sandia.gov)

**Abstract**

Nuclear engineering codes are being used to simulate more challenging problems and at higher fidelities than they were initially developed for. In order to expand the capabilities of these codes, state of the art numerical methods and computer science need to be implemented. One of the key players in this effort is the Consortium for Advanced Simulation of Light Water Reactors (CASL) and through development of the Virtual Environment for Reactor Applications (VERA). The sub-channel thermal hydraulic code used in VERA, COBRA-TF (Coolant-Boiling in Rod Arrays - Three Fluids), is partially developed at the Pennsylvania State University by the Reactor Dynamics and Fuel Management Research Group (RDFMG).

Currently, COBRA-TF solves 8 conservation equations for liquid, entrained droplet, and vapor phases of water boiling within the rod structure of a LWR reactor core. The conservation equations analytically reduce into a pressure matrix and are solved using a semi-implicit method. The solid conduction equations are then implicitly solved to determine the temperature within the fuel. Since the liquid solution is solved independent of the solid solution, the solid and liquid equations are explicitly coupled.

In an effort to help meet the objectives of CASL, a version of COBRTA-TF has been developed that solves the residual formulation of the 1D single-phase conservation equations. The formulation of the base equations as residuals allows the code to be run semi-implicitly or fully implicitly while clearly defining the original conservation equations. This paper outlines work to integrate 1D solid conduction equations into the residual formulation. This expands the solid liquid coupling to be either explicit or implicit. Different physical models, such as the homogeneous liquid solid energy model, can be readily implemented by adding the residual functions and variables. A simple test problem consisting of a single liquid channel and fuel pin was designed to compare the original version of COBRA-TF to the different numerical and physical models available through the new residual formulation. The methods are compared both for steady state and transient conditions to quantify the accuracy and stability of each method. The input parameters are varied over a variety of conditions to demonstrate when different methods are most appropriate. The ability to choose appropriate numerical methods and physical models will allow for greater fidelity, decrease computational expenses.

**Keywords:** thermal hydraulic, residual, jacobian, solid liquid coupling, COBRA-TF, PETSC